2. b. You would use edge-triggered registers because level-triggered registers allow multiple cycles of data in which would cause a clog in the system therefore with the edge-triggered registers there would only be one cycle of data at a time.