2. e. The circuit puts a constraint on how short the CPU’s clock can be due to the longer time it takes to calculate the 32-bit multiplication. If a 32-bit multiplication is continually being used on the CPU then the clock must be lengthened to accommodate the longer process time otherwise the 32-bit multiplication would need to be split into parts to shorten the process time.